|  |  |  |  |
| --- | --- | --- | --- |
| **Vessel Name :** | ENL SUPERIOR | **Reqn No:** | ENLS-2021-0224 |
| **Department :** | SHIP | **Vessel Reference :** | ENLS-2021-0224 |
| **Reqn. Date :** | 26/01/2021 | **Deliver By :** |  |
| **Requisition Type :** | REQUISITION FOR EMERGENCY FIRE PUMP DISCHARGE HOSE AND OTHERS SURVEYOR HIGHLIGHTING DEFECTS TO BE CLOSED. | **Priority :** | **URGENT (REMINDER)** |
| **Account Code :** |  | **Currency :** |  |
| Payment Terms |  | | |
| **Delivery Terms** | AT F.O.T ONNE PORT HARCOURT. | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Description:** | REQUISITION FOR EMERGENCY FIRE PUMP HOSE | **MADE:** |  |
| **For Equipment:** | EMERGENCY FIRE PUMP | MODEL: |  |
|  |  | **SERIAL:** |  |
| **Equipment Remark: REQUISITION FOR EMERGENCY FIRE PUMP HOSE , FORMER ONE IS FAULTY.** | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SR.No.** | **Part No** | **Part Name** | **Product. No/** | **Maker’s Reference** | **Unit** | **Stock** | **Qty Req.** | | **Qty approved** | **Est. Price** | **Item Remarks** |
| 1 | EN 14540.04 | REQUISITION FOR EMERGENCY FIRE PUMP HOSE.LENGTH = 20M (20,000mm) , DIAMETER = 2 INCHES, PRESSURE = 12BAR |  | DN454PV45J5847N | ROLL |  | 4 |  | |  |  |
| 2 |  | REQUISITION FOR MECHANISM FOR MESS ROOM DOOR |  |  | PSC |  | 4 |  | |  |  |
| 3 |  | REQUISITION FOR METRO ONE INSECT PEST    KILLER. AC=220V , 50/60HZT |  | BK-L20/2X10W |  |  |  |  | |  |  |
| 4 |  | REQUISITION FOR WATER CLOSET VENT (WC) WING NUT AND BOLT,WING NUT= 11 MM , BOLT = 11MM. |  |  | PSC |  | 12EACH |  | |  |  |
| 5 |  | REQUISITION FOR WATER HEATER NIPPLE, STAINLESS PIPE,LENGTH =42MM,EXTERNAL DIAMETR=23MM, INTERNAL DIAMETER=11.5MM. |  |  | PC |  | 1 |  | |  |  |
| 6 |  | REQUISITION FOR MAIN ENGINE REMOTE  INDICATOR NAME PLATE |  |  | PSC |  | 4 |  | |  |  |
| 7 |  | REQUISITION FOR FLASH LIGHT IN THE FIRE MANS OUT FIT |  |  | PSC |  | 30 |  | |  |  |
| 8 |  | REQUISITION FOR PORT ANCHOR. |  |  | PSC |  | 1 |  | |  |  |
| 9 |  | REQUISITION FOR WASTE DISPOSAL PLASTIC BUCKET BIN WITH WITH OPEN AND CLOSE MECHANISM 50LTR |  |  | PSC |  | 6 |  | |  |  |
| 10 |  | REQUISITION FOR REPAIR OF GYRO COMPASS THT NOT SYNCHRONIZED WITH RUDDER . |  |  |  |  | 1 |  | |  |  |
| 11 |  | REQUISITION FOR FIXING OF ANTIGUE HINGES FOR FIRE HOSE BOX ANTIGUE HINGES=3INCHE= 8PSC, PADLOCK HINGES =8PIECES, BOLTS AND NUT 4MM WITH WASHERS |  |  | PSC |  | 8 EACH |  | |  |  |
| 12 |  | REQUISITION FOR WELDER FOR CLOSING OF DEFECT ONBOARD. |  |  |  |  |  |  | |  |  |
| 13 |  | REQUISITION FOR SWIVEL AND SHACKLE I” |  |  | PSC |  | 3 EACH |  | |  |  |

|  |  |
| --- | --- |
| **Total in(**Naira**)** |  |

**Instructions To Vendor:**

**Comment:**