|  |  |  |  |
| --- | --- | --- | --- |
| **Vessel Name :** | ENL SUPERIOR | **Reqn No:** | ENLS-2021-0268 |
| **Department :** | ENGINE ROOM. | **Vessel Reference :** |  |
| **Reqn. Date :** | 06/04/2021 | **Deliver By :** |  |
| **Requisition Type :** | REQUISITION FOR GRINDING AND LAPPING OF NON RETURN VALVES OVER BOARD IN ENGINE ROOM. | **Priority :** | **URGENT (REMINDER)** |
| **Account Code :** |  | **Currency :** |  |
| **Payment Terms** |  | | |
| **Delivery Terms** |  | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Description:** | REQUISITION FOR GRINDING AND LAPPING | **MADE:**  **SERIAL:** |  |
| **For Equipment:** | ENGINE ROOM OVER BOARD NON RETURN VALVES. | MODEL: |  |
|  |  |  |  |
| **Equipment Remark: THERE IS NEED TO SERVICE ALL OVER BOARD NON RETURN VALVES AT DRY DOCK FOR PROPER DISCHARGING.** | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SR.No.** | **Part No** | **Part Name** | **Product. No/** | **Maker’s Reference** | **Unit** | **Stock** | **Qty Req.** | **Qty approved** | | **Est. Price** | **Item Remarks** |
|  |  | REQUISITION FOR GRINDING AND LAPPING OF OVER BOARD NON RETURN VALVES IN ENGINE ROOM. |  | SIZE’S |  |  |  | |  |  |  |
| 1 |  | BOTH MAIN ENGINES GEAR BOX OVERBOARD VALVES PORT AND STBD |  | SIZE DN50 (50.8MM) | PCS |  | 2 |  | |  |  |
| 2 |  | BOTH MAIN ENGINES SEA WATER OVERBOARD VALVES PORT AND STBD |  | SIZE 10K100 (108MM) | PCS |  | 2 |  | |  |  |
| 3 |  | GENERAL SERVICE PUMP OVERBOARD PORT SIDE |  | DN80 (83MM) | PC |  | 1 |  | |  |  |
| 4 |  | BILGES PUMP OVERBOARD |  | DN 80 (83MM) | PC |  | 1 |  | |  |  |
| 5 |  | BOTH AUXILIARY GENERATORS #1 AND #2 OVERBOARD VALVES PORT AND STARBOARD. |  | DN 50 (50.8MM) | PCS |  | 2 |  | |  |  |
| 6 |  | CHILLER OVERBOARD.PORT SIDE |  | DN50 (50.8MM) | PC |  | 1 |  | |  |  |
| 7 |  | SEWAGE OVERBOARD NON RETURN VALVE PORT SIDE. |  | DN125 (127MM) | PC |  | 1 |  | |  |  |
| 8 |  | LAUNDRY DRIAN OVERBOARD PORT SIDE. PORT SIDE. |  | DN 85 (88.7MM) | PC |  | 1 |  | |  |  |
| 9 |  | GALLEY DRAIN PORT SIDE.. |  | DN 85 ( 88.7MM) | PC |  | 1 |  | |  |  |
| 10 |  | FIFI PUMP OVER BOARD STAR BOARD SIDE. |  | 10K 100 (101.6MM) | PC |  | 1 |  | |  |  |
| 11 |  | OILY WATER SEPARATOR OVERBOARD . STARBOARD SIDE |  | DN20 (19.05MM) | PC |  | 1 |  | |  |  |
| 12 |  | AIR CONDITION OVERBOARD. STAR BOARD SIDE |  | DN40 (44.45MM) | PC |  | 1 |  | |  |  |
|  |  |  |  |  |  |  |  |  | |  |  |

**Comment:**