|  |  |  |  |
| --- | --- | --- | --- |
| **Vessel Name :** | ENL SUPERIOR | **Reqn No:** | ENLS-2021-0337 |
| **Department :** | ENGINE ROOM | **Vessel Reference :** |  |
| **Reqn. Date :** | 18-09-2021 | **Deliver By :** |  |
| **Requisition Type :** | DRY DOCK REQUISITION | **Priority :** |  |
| **Account Code :** |  | **Currency :** |  |
| **Payment Terms** |  | | |
| **Delivery Terms** |  | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Description:** | DRY DOCK REQUISITION | **MADE: CHINA** |  |
| **For Equipment:** | MISCELLENOUS | MODEL: |  |
|  |  | **SERIAL nO** |  |
| **Equipment Remark: DEFECT REPORT RECOMMENDATION REQUISITION** | | | |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **SR.No.** | **Part No** | **Name** | **Product. No/** | **Maker’s Reference** | **Unit** | **Stock** | **Qty Req.** | **Qty approved** | | **Est. Price** | **Item Remarks** |
| 1 |  | REPAIR OF OILY WATER SEPARATOR |  |  |  |  | 1PCS | | 1PCS |  | Approved for replacement of oily water separator indicator. |
| 2 |  | REPAIR/ REPLACEMENT OF QUICK CLOSE VALVES |  |  |  |  | 17PCS | | 17 PCS |  | To be serviced for all the fuel lines. |
| 3 |  | REPLACEMENT OF SEA WATER HYDROPHONE |  |  |  |  | 1 PCS | | 1PCS |  | Corroded and leaking, approved for replacement. |
| 4 |  | REPLACEMENT OF EMERGENCY FIRE PUMP STARTER |  |  |  |  | 1 PCS | | 1PCS |  | Kick Starter failing, Replacement required while the defective can be repaired as spare. |
| 5 |  | FUEL OIL PURIFIER |  | ALFA-LAVA |  |  | 1PICS | | 1 PCS |  | Approved |
| 6 |  | DENSO TAPE ( GREASE TYPE) |  |  |  |  | 2ROLL | | 1 ROLL |  | Approved |

**Instructions To Vendor:**

**Comment:**